/* A(ll) access permited
   R(ead only) access
   E(nd init protected) access

   A|R|E(offset, register, feature introducing reg)

   NOTE: PSW is handled as a special case in gen_mtcr/mfcr */

A(0xfe00, PCXI, TRICORE_FEATURE_13)
A(0xfe08, PC, TRICORE_FEATURE_13)
A(0xfe14, SYSCON, TRICORE_FEATURE_13)
R(0xfe18, CPU_ID, TRICORE_FEATURE_13)
E(0xfe20, BIV, TRICORE_FEATURE_13)
E(0xfe24, BTV, TRICORE_FEATURE_13)
E(0xfe28, ISP, TRICORE_FEATURE_13)
A(0xfe2c, ICR, TRICORE_FEATURE_13)
A(0xfe38, FCX, TRICORE_FEATURE_13)
A(0xfe3c, LCX, TRICORE_FEATURE_13)
E(0x9400, COMPAT, TRICORE_FEATURE_131)
/* memory protection register */
A(0xC000, DPR0_0L, TRICORE_FEATURE_13)
A(0xC004, DPR0_0U, TRICORE_FEATURE_13)
A(0xC008, DPR0_1L, TRICORE_FEATURE_13)
A(0xC00C, DPR0_1U, TRICORE_FEATURE_13)
A(0xC010, DPR0_2L, TRICORE_FEATURE_13)
A(0xC014, DPR0_2U, TRICORE_FEATURE_13)
A(0xC018, DPR0_3L, TRICORE_FEATURE_13)
A(0xC01C, DPR0_3U, TRICORE_FEATURE_13)
A(0xC400, DPR1_0L, TRICORE_FEATURE_13)
A(0xC404, DPR1_0U, TRICORE_FEATURE_13)
A(0xC408, DPR1_1L, TRICORE_FEATURE_13)
A(0xC40C, DPR1_1U, TRICORE_FEATURE_13)
A(0xC410, DPR1_2L, TRICORE_FEATURE_13)
A(0xC414, DPR1_2U, TRICORE_FEATURE_13)
A(0xC418, DPR1_3L, TRICORE_FEATURE_13)
A(0xC41C, DPR1_3U, TRICORE_FEATURE_13)
A(0xC800, DPR2_0L, TRICORE_FEATURE_13)
A(0xC804, DPR2_0U, TRICORE_FEATURE_13)
A(0xC808, DPR2_1L, TRICORE_FEATURE_13)
A(0xC80C, DPR2_1U, TRICORE_FEATURE_13)
A(0xC810, DPR2_2L, TRICORE_FEATURE_13)
A(0xC814, DPR2_2U, TRICORE_FEATURE_13)
A(0xC818, DPR2_3L, TRICORE_FEATURE_13)
A(0xC81C, DPR2_3U, TRICORE_FEATURE_13)
A(0xCC00, DPR3_0L, TRICORE_FEATURE_13)
A(0xCC04, DPR3_0U, TRICORE_FEATURE_13)
A(0xCC08, DPR3_1L, TRICORE_FEATURE_13)
A(0xCC0C, DPR3_1U, TRICORE_FEATURE_13)
A(0xCC10, DPR3_2L, TRICORE_FEATURE_13)
A(0xCC14, DPR3_2U, TRICORE_FEATURE_13)
A(0xCC18, DPR3_3L, TRICORE_FEATURE_13)
A(0xCC1C, DPR3_3U, TRICORE_FEATURE_13)
A(0xD000, CPR0_0L, TRICORE_FEATURE_13)
A(0xD004, CPR0_0U, TRICORE_FEATURE_13)
A(0xD008, CPR0_1L, TRICORE_FEATURE_13)
A(0xD00C, CPR0_1U, TRICORE_FEATURE_13)
A(0xD010, CPR0_2L, TRICORE_FEATURE_13)
A(0xD014, CPR0_2U, TRICORE_FEATURE_13)
A(0xD018, CPR0_3L, TRICORE_FEATURE_13)
A(0xD01C, CPR0_3U, TRICORE_FEATURE_13)
A(0xD400, CPR1_0L, TRICORE_FEATURE_13)
A(0xD404, CPR1_0U, TRICORE_FEATURE_13)
A(0xD408, CPR1_1L, TRICORE_FEATURE_13)
A(0xD40C, CPR1_1U, TRICORE_FEATURE_13)
A(0xD410, CPR1_2L, TRICORE_FEATURE_13)
A(0xD414, CPR1_2U, TRICORE_FEATURE_13)
A(0xD418, CPR1_3L, TRICORE_FEATURE_13)
A(0xD41C, CPR1_3U, TRICORE_FEATURE_13)
A(0xD800, CPR2_0L, TRICORE_FEATURE_13)
A(0xD804, CPR2_0U, TRICORE_FEATURE_13)
A(0xD808, CPR2_1L, TRICORE_FEATURE_13)
A(0xD80C, CPR2_1U, TRICORE_FEATURE_13)
A(0xD810, CPR2_2L, TRICORE_FEATURE_13)
A(0xD814, CPR2_2U, TRICORE_FEATURE_13)
A(0xD818, CPR2_3L, TRICORE_FEATURE_13)
A(0xD81C, CPR2_3U, TRICORE_FEATURE_13)
A(0xDC00, CPR3_0L, TRICORE_FEATURE_13)
A(0xDC04, CPR3_0U, TRICORE_FEATURE_13)
A(0xDC08, CPR3_1L, TRICORE_FEATURE_13)
A(0xDC0C, CPR3_1U, TRICORE_FEATURE_13)
A(0xDC10, CPR3_2L, TRICORE_FEATURE_13)
A(0xDC14, CPR3_2U, TRICORE_FEATURE_13)
A(0xDC18, CPR3_3L, TRICORE_FEATURE_13)
A(0xDC1C, CPR3_3U, TRICORE_FEATURE_13)
A(0xE000, DPM0, TRICORE_FEATURE_13)
A(0xE080, DPM1, TRICORE_FEATURE_13)
A(0xE100, DPM2, TRICORE_FEATURE_13)
A(0xE180, DPM3, TRICORE_FEATURE_13)
A(0xE200, CPM0, TRICORE_FEATURE_13)
A(0xE280, CPM1, TRICORE_FEATURE_13)
A(0xE300, CPM2, TRICORE_FEATURE_13)
A(0xE380, CPM3, TRICORE_FEATURE_13)
/* memory management registers */
A(0x8000, MMU_CON, TRICORE_FEATURE_13)
A(0x8004, MMU_ASI, TRICORE_FEATURE_13)
A(0x800C, MMU_TVA, TRICORE_FEATURE_13)
A(0x8010, MMU_TPA, TRICORE_FEATURE_13)
A(0x8014, MMU_TPX, TRICORE_FEATURE_13)
A(0x8018, MMU_TFA, TRICORE_FEATURE_13)
E(0x9004, BMACON, TRICORE_FEATURE_131)
E(0x900C, SMACON, TRICORE_FEATURE_131)
A(0x9020, DIEAR, TRICORE_FEATURE_131)
A(0x9024, DIETR, TRICORE_FEATURE_131)
A(0x9028, CCDIER, TRICORE_FEATURE_131)
E(0x9044, MIECON, TRICORE_FEATURE_131)
A(0x9210, PIEAR, TRICORE_FEATURE_131)
A(0x9214, PIETR, TRICORE_FEATURE_131)
A(0x9218, CCPIER, TRICORE_FEATURE_131)
/* debug registers */
A(0xFD00, DBGSR, TRICORE_FEATURE_13)
A(0xFD08, EXEVT, TRICORE_FEATURE_13)
A(0xFD0C, CREVT, TRICORE_FEATURE_13)
A(0xFD10, SWEVT, TRICORE_FEATURE_13)
A(0xFD20, TR0EVT, TRICORE_FEATURE_13)
A(0xFD24, TR1EVT, TRICORE_FEATURE_13)
A(0xFD40, DMS, TRICORE_FEATURE_13)
A(0xFD44, DCX, TRICORE_FEATURE_13)
A(0xFD48, DBGTCR, TRICORE_FEATURE_131)
A(0xFC00, CCTRL, TRICORE_FEATURE_131)
A(0xFC04, CCNT, TRICORE_FEATURE_131)
A(0xFC08, ICNT, TRICORE_FEATURE_131)
A(0xFC0C, M1CNT, TRICORE_FEATURE_131)
A(0xFC10, M2CNT, TRICORE_FEATURE_131)
A(0xFC14, M3CNT, TRICORE_FEATURE_131)
