(footprint "Type_C_PD_Module" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr through_hole)
  (fp_text reference "REF**" (at 0 -10.5 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 80534da7-48fa-44a0-a886-dc4dc4436175)
  )
  (fp_text value "Type_C_PD_Module" (at 0 1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 127d9941-9f61-49af-836a-f82c42887657)
  )
  (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp a5869196-9b63-4044-b616-874787bd3848)
  )
  (fp_rect (start -9 -12) (end 9 12)
    (stroke (width 0.12) (type default)) (fill none) (layer "F.CrtYd") (tstamp 8225422f-9109-476d-8d82-6c5225965288))
  (pad "" np_thru_hole circle (at -9 -8.25) (size 2 2) (drill 2) (layers "F&B.Cu" "*.Mask") (tstamp debfc415-0fb8-4afd-a886-a4f735d02a64))
  (pad "" np_thru_hole circle (at 9 -8.25) (size 2 2) (drill 2) (layers "F&B.Cu" "*.Mask") (tstamp 329e83a7-e14c-4ac5-a172-9c9de9a63f99))
  (pad "1" thru_hole oval (at -8 10.4 90) (size 3 2) (drill 0.8) (layers "*.Cu" "*.Mask") (tstamp ed11e90c-6a61-4f48-9651-b4fb3ce8cef5))
  (pad "2" thru_hole oval (at 7.9 10.4 90) (size 3 2) (drill 0.8) (layers "*.Cu" "*.Mask") (tstamp e453b380-5494-4698-9322-304116e24cd7))
)
