(footprint "HT-RA62"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -12.55 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "90168f83-941d-4cf3-bb53-2b6cdfeacb55")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "HT-RA62"
		(at 0 0.95 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "0470bbdd-4a14-4781-9e04-70bb54c77cb5")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "69729c54-1b8e-4a29-9b79-bcdafdea79e1")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "339814cd-58d3-4cb4-ba8d-cb1a08fa04fb")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_rect
		(start -9.5 -8.35)
		(end 9.5 8.65)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill no)
		(layer "F.SilkS")
		(uuid "8893dad4-9878-496b-b2ca-d8f1e661af40")
	)
	(fp_text user "${REFERENCE}"
		(at 0 2.45 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "c7f135fd-b657-4813-bd0c-d930c9b583f3")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at -8 -7)
		(size 2.5 1.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "c343e818-7fc0-4080-a431-b11d17e54678")
	)
	(pad "2" smd roundrect
		(at -8 -5)
		(size 2.5 1.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "5d9cc7df-01e5-4c2d-a2a4-a6551862718e")
	)
	(pad "3" smd roundrect
		(at -8 -3)
		(size 2.5 1.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "6f4d05b3-0660-4f34-93b0-19a816ad817a")
	)
	(pad "4" smd roundrect
		(at -8 -1)
		(size 2.5 1.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "9d3913b4-b729-4bc5-9c09-ef2e8d2d3df9")
	)
	(pad "5" smd roundrect
		(at -8 1)
		(size 2.5 1.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "68fee68d-8c27-4058-b531-043c71e4da60")
	)
	(pad "6" smd roundrect
		(at -8 3)
		(size 2.5 1.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "b96862ec-0e02-4b0e-9109-c7cdd611d512")
	)
	(pad "7" smd roundrect
		(at -8 5)
		(size 2.5 1.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "eda38f3c-3451-4e5f-abf9-78076caa5f59")
	)
	(pad "8" smd roundrect
		(at -8 7)
		(size 2.5 1.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "c86fa4b9-4436-4656-be50-725a4ea07d14")
	)
	(pad "9" smd roundrect
		(at 8 7)
		(size 2.5 1.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "9cbce2ea-b454-4a60-8f56-e176c850e352")
	)
	(pad "10" smd roundrect
		(at 8 5)
		(size 2.5 1.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "57825d94-0214-4ea7-bf1d-b67f6605bc94")
	)
	(pad "11" smd roundrect
		(at 8 3)
		(size 2.5 1.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "e64b9fc5-ae2f-42b4-9d33-ac3e354e35de")
	)
	(pad "12" smd roundrect
		(at 8 1)
		(size 2.5 1.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "15e4f50b-00ea-4f38-bc6b-2d0c037126d5")
	)
	(pad "13" smd roundrect
		(at 8 -1)
		(size 2.5 1.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "7ea9a734-f647-4bd2-a629-3d4bceb3d7e7")
	)
	(pad "14" smd roundrect
		(at 8 -3)
		(size 2.5 1.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "7eaf43c7-a57c-413e-98de-d6d878288782")
	)
	(pad "15" smd roundrect
		(at 8 -5)
		(size 2.5 1.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "e3409e43-7d35-4917-8788-ba99241b36cc")
	)
	(pad "16" smd roundrect
		(at 8 -7)
		(size 2.5 1.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "d361718d-c10b-415b-8fe7-8399837b3c7b")
	)
	(embedded_fonts no)
)
