(footprint "Murata_B966AS" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 0 -6.3 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp a1b84344-90fe-415b-bd4f-bb0180fa534e)
  )
  (fp_text value "Murata_B966AS" (at 0 6.1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 676b432b-5d47-4acf-8c47-d6ffbe740392)
  )
  (fp_text user "${REFERENCE}" (at 0 7.5 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 39c7c3c2-e568-463f-aa83-c40284f03cb3)
  )
  (fp_line (start -5.5 -5.2) (end -5.5 5.2)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 79747b85-cee6-4bea-80bc-006234df81cb))
  (fp_line (start -5.5 -5.2) (end 5.5 -5.2)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 1cce8af7-96b1-4ed0-9b55-cc75bf74be80))
  (fp_line (start -5.5 5.2) (end 5.5 5.2)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 38febf32-14e2-49d9-a6e1-07fa8f86366b))
  (fp_line (start 5.5 -5.2) (end 5.5 5.2)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp c416a14b-849b-4502-8c61-0ae874e91512))
  (fp_line (start -5.6 -5.3) (end -5.6 5.3)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp aef3f1ea-5763-4336-99fd-ad7d08d8243e))
  (fp_line (start -5.6 -5.3) (end 5.6 -5.3)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp adf2586a-cd58-4453-bef3-8be5c6a95b15))
  (fp_line (start -5.6 5.3) (end 5.6 5.3)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp a5368208-924a-4c61-b6b8-d250455f6917))
  (fp_line (start 5.6 -5.3) (end 5.6 5.3)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 86f3d6f5-ac50-40d0-a4e9-22a12892f93f))
  (pad "1" smd roundrect (at -4.025 0) (size 2.65 3.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 78b4ff98-f726-4020-bdf1-f32782384499))
  (pad "2" smd roundrect (at 4.025 0) (size 2.65 3.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp c0fb97c0-4105-4b82-bffb-3e98f3f77b62))
)
