(footprint "USB_A_Jing_C42660" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr through_hole)
  (fp_text reference "REF**" (at 0 -3 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp f75ad864-f096-4907-b31d-1a5733db4331)
  )
  (fp_text value "USB_A_Jing_C42660" (at 0 1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 8020425b-e9f3-495c-818a-7f5fd22a8d70)
  )
  (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp a382881d-447e-4c02-8a48-4f80e0b390fe)
  )
  (fp_line (start -6.6 -0.8) (end -6.6 1)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7e87feb7-0101-4554-befb-49d810a78ed2))
  (fp_line (start -6.6 -0.8) (end 6.6 -0.8)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d4f4dd60-7f1f-403d-a8be-9d541794b9e6))
  (fp_line (start -6.6 4.4) (end -6.6 13.2)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0bc4bf27-d3dc-4241-bb6c-8ffb88859a86))
  (fp_line (start -6.6 13.2) (end 6.6 13.2)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6c58bef7-a109-4acd-b484-5503636af5ac))
  (fp_line (start 6.6 -0.8) (end 6.6 1)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1e01b4d9-a989-409c-94fd-57d5171ccf78))
  (fp_line (start 6.6 4.4) (end 6.6 13.2)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 57f1b421-32fe-4316-8a13-1ecb16ddbbaf))
  (fp_rect (start -8.2 -1.2) (end 8.4 13.6)
    (stroke (width 0.12) (type solid)) (fill none) (layer "F.CrtYd") (tstamp 97b6903c-ae03-48c5-b4bb-1e6df8addd30))
  (pad "1" thru_hole circle (at 3.5 0) (size 1.2 1.2) (drill 0.9) (layers "*.Cu" "*.Mask") (tstamp bf76e491-9dd7-40e2-950e-c79b71b72d93))
  (pad "2" thru_hole circle (at 1 0) (size 1.2 1.2) (drill 0.9) (layers "*.Cu" "*.Mask") (tstamp fa3e4d8c-7c0c-49b2-8f34-dbc76c0c364e))
  (pad "3" thru_hole circle (at -1 0) (size 1.2 1.2) (drill 0.9) (layers "*.Cu" "*.Mask") (tstamp d4286bc5-3f3a-4659-80b9-42b41fa62ce8))
  (pad "4" thru_hole circle (at -3.5 0) (size 1.2 1.2) (drill 0.9) (layers "*.Cu" "*.Mask") (tstamp 280b0630-d0d3-42bc-a3bf-d42ba3faa203))
  (pad "5" thru_hole circle (at -6.57 2.71) (size 3 3) (drill 2.3) (layers "*.Cu" "*.Mask") (tstamp fb80ec7a-b41c-47ce-88ad-426f8849926c))
  (pad "5" thru_hole circle (at 6.57 2.71) (size 3 3) (drill 2.3) (layers "*.Cu" "*.Mask") (tstamp 41b2f027-a9f8-44ee-9a65-3f24b6354ad8))
)
