(footprint "AHT20"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -13.3 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "87b9ee8c-2176-4970-97b1-bcde8ccac43a")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "AHT20"
		(at 0 2.25 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "93cd5c18-6553-4121-aa20-ad9e7013470f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "a14d4b1b-ed23-43fd-8ca4-d5da47d08f79")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "5c17a7e0-438e-4698-860d-fef43acce600")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(fp_line
		(start -0.4 -1.2)
		(end -0.4 -0.85)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "100a6eb0-88ec-44fb-80f8-5c946f92d994")
	)
	(fp_line
		(start -0.4 -1.2)
		(end -0.05 -1.2)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "0e0a7cdc-181e-4a5f-9fe6-6ebd39a26a78")
	)
	(fp_line
		(start -0.4 -0.85)
		(end -0.05 -1.2)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "b5e13012-19ed-4402-8e21-3eb784f2de48")
	)
	(fp_rect
		(start -1.55 -1.4)
		(end 1.5 1.35)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill no)
		(layer "F.SilkS")
		(uuid "9e29d228-59eb-443e-98fd-0fbccedcde54")
	)
	(fp_rect
		(start -1.55 -1.4)
		(end 1.5 1.35)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "e6d9926c-d76b-4a62-9150-6f2f63a39e76")
	)
	(fp_text user "${REFERENCE}"
		(at 0 3.75 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "7355b7f5-0107-45c8-a73e-103fe035da9c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at -1 -1)
		(size 0.8 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "72d01316-fcc3-4fc9-b2ea-ad8dd446cd8e")
	)
	(pad "2" smd roundrect
		(at -1 0)
		(size 0.8 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "a5a5c25f-0082-4f01-898c-174bf67f4b0e")
	)
	(pad "3" smd roundrect
		(at -1 1)
		(size 0.8 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "1f318891-d71f-4660-8bb0-c89e22e14717")
	)
	(pad "4" smd roundrect
		(at 1 1)
		(size 0.8 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "0e8b1fd5-5275-4a23-9d4c-5db56912de82")
	)
	(pad "5" smd roundrect
		(at 1 0)
		(size 0.8 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "fe096708-d828-44d4-9b23-823b870499a2")
	)
	(pad "6" smd roundrect
		(at 1 -1)
		(size 0.8 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "540bdbc5-5838-4198-affb-a04d3afc46f2")
	)
	(embedded_fonts no)
)
