(footprint "TestPoint_1x_SOIC"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -0.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "98ece298-d295-4a80-86c9-4fe1cb6d24f5")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "TestPoint_1x_SOIC"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "abbd6b8e-fecf-4329-823e-031ac4d3ce56")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "4ae00894-a4b8-4e4f-8d39-f276b291a3d1")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "3d4e5fa0-a884-454c-b2f1-ee4491c8b733")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "cfa9f049-4d76-4728-87b5-65ef20df482a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole roundrect
		(at 0 0 270)
		(size 2 0.8)
		(drill 0.5
			(offset 1 0)
		)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "26c82491-d118-47cd-9fca-8ca36228abd8")
	)
	(embedded_fonts no)
)
