(footprint "BK-18650-PC4"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -0.3 -4.9 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "f4b5b1bd-8620-4a74-9184-48487bf027d6")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "BK-18650-PC4"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "288a0b7b-edcd-4a77-aa0e-9f3d0a597c2c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "02c99dc9-5c2f-40da-8db4-0d9ac8783278")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "e284d542-8ffc-4ce0-8762-324738c7b5e5")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(fp_rect
		(start -38.85 -20.105)
		(end 38.85 20.105)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill no)
		(layer "F.SilkS")
		(uuid "ce84f6c5-4114-40ae-8163-6144c133810d")
	)
	(fp_rect
		(start -39.85 -21.105)
		(end 39.85 21.105)
		(stroke
			(width 0.05)
			(type solid)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "59688b38-95fa-460f-8b18-975af98c59dd")
	)
	(fp_text user "${REFERENCE}"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "204e9d3d-7548-47e1-8ba8-51e7caf2257e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "" np_thru_hole circle
		(at -27.81 -9.65)
		(size 3.2 3.2)
		(drill 3.2)
		(layers "F&B.Cu" "*.Mask")
		(uuid "351d92c7-aa48-4786-a604-c025e9edd04f")
	)
	(pad "" np_thru_hole circle
		(at -27.81 9.65)
		(size 3.2 3.2)
		(drill 3.2)
		(layers "F&B.Cu" "*.Mask")
		(uuid "ccf2d72c-030a-432b-8239-a3b85ac82cbc")
	)
	(pad "" np_thru_hole circle
		(at 27.81 -9.65)
		(size 3.2 3.2)
		(drill 3.2)
		(layers "F&B.Cu" "*.Mask")
		(uuid "31889bd2-5df7-4120-aa2c-87b314a65660")
	)
	(pad "" np_thru_hole circle
		(at 27.81 9.65)
		(size 3.2 3.2)
		(drill 3.2)
		(layers "F&B.Cu" "*.Mask")
		(uuid "926b5390-32cd-4f05-bacd-faab2f23a2d8")
	)
	(pad "1" thru_hole circle
		(at -36.45 -9.65)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "4bda7dd7-36a9-4659-bed8-3fa6b8a3bfa2")
	)
	(pad "2" thru_hole circle
		(at -36.45 9.65)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "815488b7-bd67-48a5-82ce-81355a0e9076")
	)
	(pad "3" thru_hole circle
		(at 36.45 -9.65)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "471a8929-1e98-41c3-9e05-b325c6555d6a")
	)
	(pad "4" thru_hole circle
		(at 36.45 9.65)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "c97d5bf4-55e9-4c66-936d-be7400a83998")
	)
	(embedded_fonts no)
)
