(footprint "Amphenol_YK3210203000G" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr through_hole)
  (fp_text reference "REF**" (at 0 -6.7 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp bfe8e976-f96e-4681-bbea-7ba4834f908b)
  )
  (fp_text value "Amphenol_YK3210203000G" (at 0 2.3 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp dec05c42-09e0-4164-9734-b72e3a8f442c)
  )
  (fp_text user "${REFERENCE}" (at 0 4.3 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 973e56c4-77bb-448f-85d5-efc9b01f2cf3)
  )
  (fp_rect (start -8.05 -5.5) (end 8.05 5.5)
    (stroke (width 0.12) (type default)) (fill none) (layer "F.SilkS") (tstamp 84cea2fb-1ccd-4899-bfcc-b11186af5494))
  (fp_rect (start -8.2 -5.6) (end 8.2 5.6)
    (stroke (width 0.05) (type default)) (fill none) (layer "F.CrtYd") (tstamp 48613c02-0c4d-4157-b653-7d4c50e48c5c))
  (pad "1" thru_hole circle (at -3.81 0) (size 3 3) (drill 2) (layers "*.Cu" "*.Mask") (tstamp ce00be2d-62ff-44b8-bfa5-fcb447f9b07c))
  (pad "2" thru_hole circle (at 3.81 0) (size 3 3) (drill 2) (layers "*.Cu" "*.Mask") (tstamp d9d310aa-9d9d-48a3-b1b3-1f1631eb2e03))
)
