(module QFN-42-1EP_9x3.5mm_P0.5mm_EP7x1.8mm (layer F.Cu) (tedit 6461BD03)
  (descr "QFN, 42 Pin (https://www.diodes.com/assets/Datasheets/PI3WVR12412.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
  (tags "QFN NoLead")
  (attr smd)
  (fp_text reference REF** (at 0 -3.08) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value QFN-42-1EP_9x3.5mm_P0.5mm_EP7x1.8mm (at 0 3.08) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 4.41 -1.86) (end 4.61 -1.86) (layer F.SilkS) (width 0.12))
  (fp_line (start 4.61 -1.86) (end 4.61 -1.16) (layer F.SilkS) (width 0.12))
  (fp_line (start -4.41 1.86) (end -4.61 1.86) (layer F.SilkS) (width 0.12))
  (fp_line (start -4.61 1.86) (end -4.61 1.16) (layer F.SilkS) (width 0.12))
  (fp_line (start 4.41 1.86) (end 4.61 1.86) (layer F.SilkS) (width 0.12))
  (fp_line (start 4.61 1.86) (end 4.61 1.16) (layer F.SilkS) (width 0.12))
  (fp_line (start -4.41 -1.86) (end -4.61 -1.86) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.625 -1.75) (end 4.5 -1.75) (layer F.Fab) (width 0.1))
  (fp_line (start 4.5 -1.75) (end 4.5 1.75) (layer F.Fab) (width 0.1))
  (fp_line (start 4.5 1.75) (end -4.5 1.75) (layer F.Fab) (width 0.1))
  (fp_line (start -4.5 1.75) (end -4.5 -0.875) (layer F.Fab) (width 0.1))
  (fp_line (start -4.5 -0.875) (end -3.625 -1.75) (layer F.Fab) (width 0.1))
  (fp_line (start -5.12 -2.38) (end -5.12 2.38) (layer F.CrtYd) (width 0.05))
  (fp_line (start -5.12 2.38) (end 5.12 2.38) (layer F.CrtYd) (width 0.05))
  (fp_line (start 5.12 2.38) (end 5.12 -2.38) (layer F.CrtYd) (width 0.05))
  (fp_line (start 5.12 -2.38) (end -5.12 -2.38) (layer F.CrtYd) (width 0.05))
  (pad 1 smd roundrect (at -4.4375 -0.75) (size 0.875 0.3) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 2 smd roundrect (at -4.4375 -0.25) (size 0.875 0.3) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 3 smd roundrect (at -4.4375 0.25) (size 0.875 0.3) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 4 smd roundrect (at -4.4375 0.75) (size 0.875 0.3) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 5 smd roundrect (at -4 1.6875) (size 0.3 0.875) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 6 smd roundrect (at -3.5 1.6875) (size 0.3 0.875) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 7 smd roundrect (at -3 1.6875) (size 0.3 0.875) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 8 smd roundrect (at -2.5 1.6875) (size 0.3 0.875) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 9 smd roundrect (at -2 1.6875) (size 0.3 0.875) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 10 smd roundrect (at -1.5 1.6875) (size 0.3 0.875) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 11 smd roundrect (at -1 1.6875) (size 0.3 0.875) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 12 smd roundrect (at -0.5 1.6875) (size 0.3 0.875) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 13 smd roundrect (at 0 1.6875) (size 0.3 0.875) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 14 smd roundrect (at 0.5 1.6875) (size 0.3 0.875) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 15 smd roundrect (at 1 1.6875) (size 0.3 0.875) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 16 smd roundrect (at 1.5 1.6875) (size 0.3 0.875) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 17 smd roundrect (at 2 1.6875) (size 0.3 0.875) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 18 smd roundrect (at 2.5 1.6875) (size 0.3 0.875) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 19 smd roundrect (at 3 1.6875) (size 0.3 0.875) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 20 smd roundrect (at 3.5 1.6875) (size 0.3 0.875) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 21 smd roundrect (at 4 1.6875) (size 0.3 0.875) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 22 smd roundrect (at 4.4375 0.75) (size 0.875 0.3) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 23 smd roundrect (at 4.4375 0.25) (size 0.875 0.3) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 24 smd roundrect (at 4.4375 -0.25) (size 0.875 0.3) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 25 smd roundrect (at 4.4375 -0.75) (size 0.875 0.3) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 26 smd roundrect (at 4 -1.6875) (size 0.3 0.875) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 27 smd roundrect (at 3.5 -1.6875) (size 0.3 0.875) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 28 smd roundrect (at 3 -1.6875) (size 0.3 0.875) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 29 smd roundrect (at 2.5 -1.6875) (size 0.3 0.875) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 30 smd roundrect (at 2 -1.6875) (size 0.3 0.875) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 31 smd roundrect (at 1.5 -1.6875) (size 0.3 0.875) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 32 smd roundrect (at 1 -1.6875) (size 0.3 0.875) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 33 smd roundrect (at 0.5 -1.6875) (size 0.3 0.875) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 34 smd roundrect (at 0 -1.6875) (size 0.3 0.875) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 35 smd roundrect (at -0.5 -1.6875) (size 0.3 0.875) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 36 smd roundrect (at -1 -1.6875) (size 0.3 0.875) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 37 smd roundrect (at -1.5 -1.6875) (size 0.3 0.875) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 38 smd roundrect (at -2 -1.6875) (size 0.3 0.875) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 39 smd roundrect (at -2.5 -1.6875) (size 0.3 0.875) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 40 smd roundrect (at -3 -1.6875) (size 0.3 0.875) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 41 smd roundrect (at -3.5 -1.6875) (size 0.3 0.875) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 42 smd roundrect (at -4 -1.6875) (size 0.3 0.875) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 43 smd rect (at 0 0) (size 7 1.8) (layers F.Cu F.Mask))
  (pad "" smd roundrect (at 0 0) (size 5.64 1.45) (layers F.Paste) (roundrect_rratio 0.172414))
  (fp_text user ${REFERENCE} (at 0 0) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (model ${KICAD7_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-42-1EP_9x3.5mm_P0.5mm_EP7x1.8mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
