(footprint "LGA1151_Cooler_Mounting" (version 20210424) (generator pcbnew) (layer "F.Cu")
  (tedit 60BB8AD3)
  (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 9cafdc30-2380-457c-90c3-e270b270f5d5)
  )
  (fp_text value "LGA1151_Cooler_Mounting" (at 0 1 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp c0cdc322-4d40-4b9a-bab7-91731d7c8943)
  )
  (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 0c5dca48-5f25-43f1-a76f-29dbcf5f222c)
  )
  (fp_circle (center -37.5 37.5) (end -31.5 37.5) (layer "B.CrtYd") (width 0.12) (fill none) (tstamp ac659e5f-d113-4c30-b526-5a57042a94ae))
  (fp_circle (center 37.5 -37.5) (end 43.5 -37.5) (layer "B.CrtYd") (width 0.12) (fill none) (tstamp b2840e47-b005-46a7-90aa-6ce34aec0526))
  (fp_circle (center 37.5 37.5) (end 43.5 37.5) (layer "B.CrtYd") (width 0.12) (fill none) (tstamp fb7c888d-5eb9-4660-b4b9-a1d35e265b9c))
  (fp_circle (center -37.5 -37.5) (end -31.5 -37.5) (layer "B.CrtYd") (width 0.12) (fill none) (tstamp fcb82342-630e-4be8-be1e-e82996488456))
  (fp_circle (center 37.5 -37.5) (end 43.5 -37.5) (layer "F.CrtYd") (width 0.12) (fill none) (tstamp 084000f0-7b4b-49eb-935e-ee3e665df259))
  (fp_circle (center 37.5 37.5) (end 43.5 37.5) (layer "F.CrtYd") (width 0.12) (fill none) (tstamp 1f23df02-a4e9-44a2-9846-5728e97967a8))
  (fp_circle (center -37.5 -37.5) (end -31.5 -37.5) (layer "F.CrtYd") (width 0.12) (fill none) (tstamp 4aeae1cb-daba-40b9-b83e-e49904a3bdb0))
  (fp_circle (center -37.5 37.5) (end -31.5 37.5) (layer "F.CrtYd") (width 0.12) (fill none) (tstamp 4d4b6ab2-7bed-4eee-b29c-2a0a62497c8d))
  (fp_circle (center 0 0) (end 17.5 0) (layer "F.Fab") (width 0.12) (fill none) (tstamp f487c6d2-f1ca-48bb-997e-e75429b438e8))
  (pad "" np_thru_hole circle (at 37.5 37.5) (size 4 4) (drill 4) (layers F&B.Cu *.Mask) (tstamp 12a1a5ec-4b66-4f27-9bb5-7c933a88747c))
  (pad "" np_thru_hole circle (at -37.5 -37.5) (size 4 4) (drill 4) (layers F&B.Cu *.Mask) (tstamp 3982eed8-438f-4aaf-9496-071af0006218))
  (pad "" np_thru_hole circle (at -37.5 37.5) (size 4 4) (drill 4) (layers F&B.Cu *.Mask) (tstamp 3a62c534-7a95-47b1-8d17-2028c4cf3f9f))
  (pad "" np_thru_hole circle (at 37.5 -37.5) (size 4 4) (drill 4) (layers F&B.Cu *.Mask) (tstamp de153c7e-70f1-4739-9044-c36b77fe0543))
)
