(footprint "Hroparts_TF-01A" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 0)
  (attr smd)
  (fp_text reference "REF**" (at 0 4.3 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 55fd7d76-518e-4bd7-9c42-bc3d164b4519)
  )
  (fp_text value "Hroparts_TF-01A" (at 0 -0.1 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp bf204be1-24ec-4026-9501-6f6144432909)
  )
  (fp_text user "${REFERENCE}" (at 0 1.5 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 963fb782-498b-49b0-bfac-d2bb84fa7944)
  )
  (fp_line (start -7.8 2.3) (end -7.8 -5.5) (layer "F.SilkS") (width 0.12) (tstamp 1abd3511-2cc4-4933-9329-cb7dffb72f22))
  (fp_line (start -7.8 -7.4) (end -7.1 -7.4) (layer "F.SilkS") (width 0.12) (tstamp 250aa34a-6f8a-4b02-a1f4-1e63e70b8362))
  (fp_line (start -7.8 4.5) (end -7.8 6.5) (layer "F.SilkS") (width 0.12) (tstamp 4240f786-4bc1-430b-b11e-75257347910d))
  (fp_line (start 7.8 6.5) (end 7.8 4.5) (layer "F.SilkS") (width 0.12) (tstamp 86fa974f-c10d-48cf-9e58-9d4962446e51))
  (fp_line (start -7.8 6.5) (end 7.8 6.5) (layer "F.SilkS") (width 0.12) (tstamp c3dedb00-e397-49fc-95b8-6046e3de56fb))
  (fp_line (start 7.8 2.3) (end 7.8 -7.4) (layer "F.SilkS") (width 0.12) (tstamp d0a1089c-89b9-4266-9192-0d008876e1d5))
  (fp_line (start -7.8 -7.1) (end -7.8 -7.4) (layer "F.SilkS") (width 0.12) (tstamp dfee2a5d-4607-46aa-841d-fc383c5148f9))
  (fp_line (start 2.6 -7.4) (end 7.8 -7.4) (layer "F.SilkS") (width 0.12) (tstamp eb744c4d-13c8-445e-9fe6-5349cab0c004))
  (fp_line (start -8.6 9.4) (end 8.6 9.4) (layer "F.CrtYd") (width 0.05) (tstamp 5b8d6492-175a-47b2-a81d-2ad16d7fb405))
  (fp_line (start -8.6 -8.1) (end 8.6 -8.1) (layer "F.CrtYd") (width 0.05) (tstamp 901c79e4-f96d-4bea-bad2-1e48143567bd))
  (fp_line (start -8.6 9.4) (end -8.6 -8.1) (layer "F.CrtYd") (width 0.05) (tstamp b6841ef7-ef09-418c-b573-1487d0656fe1))
  (fp_line (start 8.6 -8.1) (end 8.6 9.4) (layer "F.CrtYd") (width 0.05) (tstamp d0e9c1f7-e760-4dbf-ae89-94ddb19e59e4))
  (pad "1" smd roundrect (at 2.14 -7.2) (size 0.7 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 5996eef6-18d9-476f-8c44-b31da3506dee))
  (pad "2" smd roundrect (at 1.04 -7.2) (size 0.7 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 2d3ff266-3de7-46b8-bab0-61a071f24d8d))
  (pad "3" smd roundrect (at -0.06 -7.2) (size 0.7 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp d0a43e83-2d0e-4efc-9e63-ef5ffe5f7d51))
  (pad "4" smd roundrect (at -1.16 -7.2) (size 0.7 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 072f2ca4-856f-45e0-9926-7bc9f3741f61))
  (pad "5" smd roundrect (at -2.26 -7.2) (size 0.7 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 689fa6fe-baef-456e-98d6-a27c3d30a5ba))
  (pad "6" smd roundrect (at -3.36 -7.2) (size 0.7 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 747f409d-9aa1-4696-ab76-4bc1bcdb3d40))
  (pad "7" smd roundrect (at -4.46 -7.2) (size 0.7 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp dd2615f8-3df5-49f3-9388-9dfd94614198))
  (pad "8" smd roundrect (at -5.56 -7.2) (size 0.7 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 5a7f0fd3-cbc5-482a-ab90-fee368e4de1c))
  (pad "10" smd roundrect (at -6.66 -7.2) (size 0.7 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp d29d9e6c-6e4b-42d3-b1b9-5ce405972e72))
  (pad "11" smd roundrect (at 6.92 -6.3) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 093dcc07-98a3-4449-98c0-e4ce6b498baf))
  (pad "11" smd roundrect (at 7.76 3.4) (size 1.2 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 1305a82d-86ed-456d-9526-078ca2b971b2))
  (pad "11" smd roundrect (at -7.76 3.4) (size 1.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 7db8bf76-eaad-41ae-a0f5-574e9cdd7be3))
  (pad "11" smd roundrect (at -7.76 -6.3) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 9b6f4cb1-82b7-4460-a53a-01279a3a43c6))
)
